**Multi-line basic insert, arranged side by side**

For buildings without a basement

For the feeding in and sealing of supply lines (power, water, telecommunications or gas) through the base slab. The two supply lines are arranged side by side.

Dimensions: Width: 216 mm; Length: 337 mm; Height: 270 mm

Material: Wall sleeve frame parts: ABS; Installation fixture: St37

Application range: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Tests/Standards: DVGW VP 601

Features: Variable height adaptation to the finished floor level; easy integration of the vapour barrier using the adhesive ribbon

Article Code: MSH Basic FUBO SR2 EBT

GTIN: -

Brand: Hauff-Technik

**Technical drawings**

[Maße MSH Basic FUBO SR2 (.PDF)](https://db.hauff-technik.de/files/1022/3/BEMA_UNG_FUBO_SR2.PDF)

Ctrl + click on the link to open in your browser

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch