**Cement-coated wall sleeve**

with special coating

Easy installation in formwork, sealed on both sides ready for installation for flush setting in concrete. Special coating creates a tight bond with the building and balances out temperature variations. From a length of > 600 mm the cement-coated pipe has a 250 mm coating on each side. Tested according to FHRK test basis with FHRK quality seal.

Material: Pipe: PVC-U; Closing cover: PE

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight

Features: Special coating creates a homogeneous bond with the concrete

Article Code: ZVR

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch