**Renovation wall sleeve**

For retrofit installation in brickwork or concrete walls.

Dimensions: Wall thickness: 4, 5 and 6 mm

Material: Pipe: PVC-U

Application range: Waterproof concrete stress class 1 and 2

Article Code: SFR

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch