**Earthing fixed point**

with weld groove

Earthing fixed point for earthing connection via weld groove, for installation flush with formwork.

Dimensions: Conductor core: round, Ø 25 mm; Contact washer: Ø 72 mm; Groove for weld connection for round steel: 10 - 12 mm; Distance between contact washer and weld groove: 40/50 or 70 mm

Material: Conductor core and contact washers: stainless steel V4A (AISI 316L); Weld connection with groove: St37

Application range: Waterproof concrete stress class 1 and 2

Tests/Standards: Short-circuit-tested to VDE 0101; EN 50522

Features: Patented twist resistance provided by special contour of contact washer

Article Code: HEA A

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch