**Standard press seal**

with graduated super segmented ring technology

Split press seal for sealing new media pipes/ducts to be installed or media pipes/ducts that have already been laid in core drills or wall sleeves. Tested according to FHRK test basis with FHRK quality seal.

Dimensions: Sealing width: 40 mm

Material: Press plates, screws and nuts: rust-free stainless steel V2A (AISI 304L) or V4A (AISI 316L); Rubber: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon tight

Features: optical and tangible installation security due to integrated control opening; Integrated super segmented ring technology for individual adjustment to cable diameter on site; Segments with exact diameter marking

Article Code: HSD SSG

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch