**Double wall insert**

adjustable length, for setting in concrete

Double wall insert for installation flush with formwork, used for the gastight and watertight connection on both sides of system seals for cables and cable ducts. Package formation is possible on site. Suitable for use in double walls/element walls.

Dimensions: Frame dimensions: 220x 220 mm; Centre distance: 210 mm; Minimum wall thickness: 200 mm

Material: Wall insert: ABS with TPE 3-ribbed seal; Adapter pipe: PVC; Clamping strap: Steel St sn (W1); Closing cover: ABS with TPE seal

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 2.5 bar; radon tight

Features: Stepless adjustment to the required wall thickness on site; In total, three spray applications of 3-ribbed seal are applied to create a pressure-tight seal with the concrete; Quality mark on both sides: sealed ex works. Option to check for accidental or unauthorised opening of the closing cover

Article Code: HSI150 K2 Varia

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch