**Earthing entry**

for retrofit installation

Earthing entry for existing walls with perimeter insulation. The seal with the wall is made on both sides with a flat gasket which is pressed against the wall with nuts. A terminal lug with cross-clamp is used to connect flat and/or round steels.

Dimensions: Contact washer: Ø 72 mm; Conductor core: M16 threaded rod; Required drill hole: 20 mm; For wall thicknesses up to 400 mm, thicker walls on request; For perimeter insulation: up to 200 mm

Material: All metal parts: stainless steel V4A (AISI 316L); Seal: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tests/Standards: DIN 18014; DIN EN 62305-3; VDE 0185-305-3 (with lightning protection application)

Article Code: HEA ND

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch