**Standard press seal**

for building connections

Press seal for sealing cables/media pipes in core drills or wall sleeves. Closed design for sealing new lines to be installed. Tested according to FHRK test basis with FHRK quality seal.

Dimensions: Sealing width: 40 mm; For core drills/wall sleeves Ø: 100 mm; For 5 cables/pipes of which 4 x Ø 7-12 mm and 1 x Ø 24-44 mm

Material: Press plates, screws and nuts: rust-free stainless steel V2A (AISI 304L); Rubber: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon tight

Features: optical and tangible installation security due to integrated control opening; Integrated segmented ring technology for individual adjustment to cable diameters on site

Article Code: HSD100 EW 1x24-44+4x7-12 b40 A2/EPDM55

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch