**Modular seal**

Modular pipe seal

Press seal for sealing new pipes to be installed or pipes that have already been laid in core drills or wall sleeves.

Material: Rubber: EDPM or NBR; Screws and nuts: rust-free stainless steel V4A (AISI 316L); Press plates: glass fibre reinforced polyamide

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon tight

Features: With integrated installation control - no torque control key required; No retightening required; Nuts moulded into the pressure plate, therefore no loose parts

Article Code: GKD

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch