**KG-FIX**

Wall collar

Water barrier flange for water pressure-tight integration of waste water pipelines in floor slabs.

Material: ABS/TPE

Application range: Waterproof concrete stress class 1 and 2

Tightness: Pressure tight up to 5,0 bar ≙ 50 m water column; radon tight

Features: Quick, tool-less assembly

Article Code: KGF

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch