**Universal wall entry**

without hem for installation in double walls/element walls

Wastewater wall entry for setting in concrete in double walls/element walls. With plug-in socket moulded on one side and three 3-ribbed seals as a water barrier in each layer of concrete.

Dimensions: DN 110: minimum wall thickness 240 mm; DN 150: minimum wall thickness 300 mm

Material: Rubber sleeve and 3-ribbed seals: EPDM; Sleeve cover: ABS; Clamping strap: Steel St sn (W1); Lamella plugs: PE; KG pipe: PVC-U/KG 2000 pipe: PP

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon tight

Tests/Standards: KG 2000 pipes to DIN EN 14758; KG pipes to DIN EN 13476-2

Features: with integrated flange connection; No change in flow direction

Article Code: UDME

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch