**Compensating attachable duct collar**

with segmented rings

Closed sealing sleeve for dowel-fitting/screwing down to outside of building/housings with existing wall sleeves, break-throughs or concrete core drills for sealing new media pipes/ducts to be installed.

Dimensions: Outer diameter ADM150: 290 mm; Outer diameter ADM200: 340 mm

Material: Sealing sleeve: EPDM; Dowel ring: stainless steel V2A (AISI 304L); Clamping straps: stainless steel V2A (AISI 304L); Fastenings: stainless steel V4A (AISI 316L)

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight

Features: Absorption of radial and axial movements; Segmented ring technology for adjustment to three or five different pipe diameters on site

Article Code: ADM

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch