**Individual press seal**

with segmented ring technology

For sealing cables in core drills or wall sleeves. Split design for sealing new cables to be installed or cables that have already been laid. The number of cables and cable diameters can be selected on an individual basis.

Dimensions: Sealing width: 40 mm; Press plates: 5 mm; Available for core drills/wall sleeves Ø: 50 - 200 mm

Material: Press plates, screws, nuts and washers: rust-free stainless steel V2A (AISI 304L) or V4A (AISI 316L); Rubber: EDPM or NBR

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon tight

Features: Tailor-made to meet requirements; Segmented ring technology for adjustment to three or five different pipe diameters on site

Article Code: HRD SGi b40

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch