**Single-line building package**

for buildings with a basement

Building package in the form of a single-line building entry system suitable for gas, water or power supplies - can used in all common types of wall. Comprising: ESH PolySafe GV1 single-purpose house entry system External sealing element ESH PolySafe M6.2 Pipe connection/extension set for MSH and ESH Basic, consisting of 1 pipe connection set (1 double socket DN75 + 3 profile seals DN75) RAS4 Universal sealing element for drinking water SDW 1x32/40/50 Universal sealing element Elektro SDE 1/26-29, 36-39, 43-46, 48-51 Universal sleeve caps MS78U 1x24-52 Insulating washer ESH PolySafe M3 for insertion into existing perimeter insulation Tube of lubricant GMT

Dimensions: Compatible with core drill/wall sleeve ID: 99 - 103 mm; Sleeve pipe OD: 75 mm, 600 mm long; maximum wall thickness: 500 mm

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar; radon tight

Tests/Standards: DVGW VP 601

Features: One-stop all-round worry-free package; optical and tangible installation security due to integrated control opening

Article Code: ESH PolySafe BHP

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch