**DiSan**

granulated, mineral sand sealant

Granulated, mineral sand sealant as a renovation solution for subsequent waterproofing of substations.

Material: mineral compound made from various sands and bentonite with optimal grain size 0/2 mm

Features: after contact with water it forms a highly plastic mixture, which provides a durable sealant for exterior areas.

Article Code: DiSan

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch