**Above-ground building entry**

for glass fibre empty conduits of 7 - 12 mm

Features: Universal building entry for drill holes in the most common types of wall. Enables horizontal or angled installation up to a 45° angle. Low-impact sealing of fibre optic cables by means of sealant.

Material: Wall terminator element: Flame-retardant polycarbonate; Pipe fastening ring: PA; Pipe fastening clip: PC; Screws: stainless steel V2A (AISI 304L)

Article Code: 2LINE OHE 1x7-12 SET10

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch