**Split system cover**

for retrofit sealing

For use in wall insert and polymer flange HSI150. Split design for sealing new cables to be installed or cables that have already been laid.

Dimensions: Sealing width: 40 mm; Press plates with reinforcement ribs: 20 mm

Material: Press plates: glass fibre reinforced polyamide; Rubber: EPDM; Screws and nuts: rust-free stainless steel V4A (AISI 316L)

Tightness: gastight and watertight to 2.5 bar; radon tight

Features: Super segmented ring technology for individual adjustment to cable diameters on site; Segments with exact diameter marking; Press plates have form-fit connections

Article Code: HSI150 DG

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch