**BD-Fix**

Slab entry

For connecting KG/HT pipes. Gastight and watertight connection to the slab thanks to integrated water barrier flange.

Material: KG pipe: PVC-U/KG 2000 pipe: PP; ABS/TPE

Application range: Waterproof concrete stress class 1 and 2

Tightness: Pressure tight up to 5,0 bar ≙ 50 m water column; radon tight

Features: Ready for installation in the slab

Article Code: BDF

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch