**PE corrugated pipe**

For ETGAR BHP

Empty conduit system for extending the ETGAR building developer package for building services outlets.

Dimensions: OD: 75 mm

Material: PE

Tightness: gastight and watertight to 0.5 bar

Features: High degree of flexibility thanks to narrow radii

Article Code: HAB ETGAR WR75 GR30000

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch