**House connection set**

for setting in concrete

Dimensions: Frame dimensions: 145x 145 mm (per wall insert); Sealing width: 40 mm; For 2 cables/pipes with 1x Ø 4.6-10.6 mm and 1x Ø 10-33 mm

Material: Wall insert: ABS with EPDM 3-ribbed seal; Adapter pipe: PVC; Closing cover: ABS with EPDM seal; Pipe cover: PE or sleeve cap: PVC; Press plates, screws and nuts: rust-free stainless steel V2A (AISI 304L); Rubber: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 0.5 bar

Features: The K55 empty conduit can be easily inserted, does not shrink, requires 2" steel pipe; Pressure-tight closing cover ensures it is gas and watertight even after the empty conduit has been connected; 3-ribbed seal is sprayed on to create pressure-tight seal with concrete

Article Code: K55/X

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch