**Standard press seal**

with segmented ring technology

Annular space seal for sealing cables in cable conduit systems, core drillings or casing pipes. Split design for sealing new cables to be installed or cables that have already been laid.

Dimensions: Sealing width: 40 mm; Press plates: 5 mm

Material: Press plates, screws, nuts and washers: rust-free stainless steel V2A (AISI 304L), (V4A (AISI 316L) on request); Rubber: EPDM

Tightness: gastight and watertight; radon tight

Features: Standard sizes suitable for Swiss cable duct systems; Segmented ring technology for adjustment to three or five different pipe diameters on site; Available from stock

Article Code: HRD SGi b40 A2/EPDM55

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch