**ETGAR building package for multi-line building service outlets**

for buildings with a basement

For routing and distributing electric power and communication lines from the building to the property's surrounding grounds.

Dimensions: Compatible with ETGAR wall sleeve, ID: 200 mm; maximum wall thickness: 500 mm

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Features: Complete system for distributing the power supply to the entire property from the building connection room; Integrated leak test equipment

Article Code: HAW-M ETGAR BHP

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch