**System cover**

with sleeve method for smooth cable ducts

System cover. Seal is both mechanically stable and elastic. Tested according to FHRK test basis with FHRK quality seal.

Material: System cover: polycarbonate; Clamping nut: PC/PBT blend; Sleeve: EPDM; Clamping straps: W4

Tightness: gastight and watertight to 0.5 bar

Features: Mechanical fixing (bayonet) and seal (clamping nut) act independently; Bayonet system with return lock and locking screw connection (for protection against automatic opening)

Article Code: HSI150 MA GR

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch