**Fire protection kit S90**

for HSI150 press seal

Fire protection kit for installation in the HSI150 system for walls. No additional wall attachments, no limits on individual cable diameters, weatherproof.

Dimensions: Wall thickness at and above: 150 mm; Barrier thickness: min. 280 mm; Maximum package size: 430 x 1270 mm (2x6)

Tests/Standards: DIBT approval Z-19.15-1906 to DIN 4102-9

Features: Fire protection S90 combined with HRD 150/160 press seal; Special assembly pockets for the assembly of pads on one side

Article Code: HSS150 HSI150 HRD

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch