**System cover**

cable seal with hot shrink-fit method

System cover. The thermal sleeves support a wide area of application, they are shrunk onto the cables by means of the application of heat from the system cover socket.

Material: System cover with socket: polycarbonate; Clamping nut: PC/PBT blend; Thermal sleeve with hot-melt adhesive: polyolefin; Centring strap: EPDM

Tightness: gastight and watertight to 2.0 bar

Features: Mechanical fixing (bayonet) and seal (clamping nut) act independently; Bayonet system with return lock and locking screw connection (for protection against automatic opening)

Article Code: HSI90 D WS

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch