**Wall collar**

Water barrier flange for water pressure-tight integration of pipelines in floor slabs.

Material: Water barrier flange: EPDM; Clamping straps: W2

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon tight

Article Code: HMK

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch