**Spiral hose system**

flexible duct system for MSH/ESH Basic FUBO

For single and multi-utility building entries, for the creation of a universal duct system up to the main supply lines. Welded-on sleeve pipe with 3-ribbed seal for connection to basic building entry units for buildings without a basement.

Dimensions: Øi: 78 mm; Øa: 87 mm

Material: Sleeve pipe and spiral hose: PVC; 3-ribbed seal: EPDM

Tightness: gastight and watertight to 1.0 bar

Features: Duct system checked for pressure tightness from the factory; including sleeve pipe and mounted 3-ribbed seal

Article Code: Hateflex14078 MRDx

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch