**ETGAR connection sleeve**

for ETGAR foundation box

For ETGAR building services outlets and for sealing media lines on the earth side at the end of the empty conduit route DA 75 mm.

Dimensions: Area of application: 1 cable OD 13 - 21 mm, 3 cables OD 7 - 13 mm, 1 cable OD 5 - 13 mm

Material: EPDM

Features: With segments for maximum area of application

Article Code: ETGAR ANS 4x5-25

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik Swiss AG**

**Manufacturer information**

Hauff-Technik Swiss AG
Grabenackerstrasse 7
4702 Oensingen, SWITZERLAND

Telefon +41 62 206 00-70
Fax +41 62 206 00-79
htch.anfrage@hauff-technik.ch
http://www.hauff-technik.ch